#

Manual Reference Pages - plan (n)

### NAME

> plan - path analysis tool

> Part of Tina Toolbox for analysis of Petri nets and Time Petri nets.

### CONTENTS

> Synopsis
> Description
> Options
> Examples
> Notes
> See Also
> Authors

### SYNOPSIS

> plan [-help]
> [-A | -S] [-t s] [-p]
> [-NET | -NDR | -PNML | -TPN | -TTS]
> [-v | -q | -s] [-abs | -rel] [-raw | -min | -can]
> [scninfile] [netinfile] [outfile] [errorfile]

### DESCRIPTION

> From a Time Petri net or Time Transition System and a firing sequence in .scn format, plan computes an inequation system characterizing all the times at which transitions in the sequence may fire, or an example firing schedule (also called path).

### OPTIONS

> -help | Recalls options.
> Operating mode options:
> -A | Returns an inequation system characterizing the times at which transition in the input .scn firing sequence may fire. If the input firing sequence is timed, then times are forgotten. Fails if the input firing sequence is not firable.
> -S | Returns a solution of the system computed by -A.
> Path options:
> -abs | Returns path system or path expressed in terms of dates (absolute times). Variable start is the time at which the initial marking is established.
> -rel | Returns path system or path expressed in terms of delays (relative times).
> -raw | Returns path system "as computed", without any particular post processing.
> -can | Returns path system in which all constraints are tight. All missing constraints, if any, are redundant and can be recovered as linear combinations of the existing constraints.
> -min | (IN PROGRESS) As -can, except that attempts to return a system without redundant constraints.
> Output format flags:
> -v | verbose output. Prints results in explicit form.
> -q | Prints a summary of results. For -A, and when -can or -min is passed, prints the duration of the shortest and longest paths. For -S, prints the duration of the path computed.
> -s | Output results in a format loadable into the nd stepper, for replaying it (only for mode -S).
> Other flags:
> -p | Disables path analysis (just parses).
> Input format flags for net:
> -NET | -NDR | -PNML | -TPN | -TTS
> | Specifies the format of the input net. This flag is necessary when the input net is read on standard input, or read from a file that does not bear the expected extension. By default, the net is assumed in .net or .ndr format.
> Firing sequence input source:
> scninfile
> | Where the firing sequence is read. If absent or specified by "-", the sequence is read on standard input.
> Net input source:
> netinfile
> | Where the net is read. The input format is determined by the file type, according to the table below. If absent or specified by "-", and the firing sequence is not read on standard input, the net is read on standard input in the format specified by the input flag. If both an infile and some input flag are present, then the format defined by the input flag supersedes that determined by the infile extension.
>     file extension          input format
>     --------------------------------------------------------------
>     .net                    net format
>     .ndr                    ndr format
>     .tpn                    tpn format
>     .pnml                   pnml format
>     .tts                    tts format
> Output destination:
> outfile
> | Where results are written. The output format is determined by the file type, according to the table below. If absent or specified by "-", then the net is written on standard output in the format specified by the output format flag. If both an outfile and some output flag are present, then the format defined by the output flag supersedes that determined by the outfile extension.
>     file extension          output format
>     --------------------------------------------------------------
>     .scn                    nd stepper format
>     any other               textual output (default -v style)
> Errors destination:
> errorfile
> | Where error messages are written. By default, errors are printed on standard error.
> Default options:
> | plan -A -v

### EXAMPLES

>     plan -A nets/ifip.scn nets/ifip.ndr
>     plan -S nets/ifip.scn nets/ifip.ndr -s
>     cat nets/ifip.scn | plan -S - nets/ifip.ndr

### NOTES

> Tool plan is still in progress; more options to come.

### SEE ALSO

> nd(n), tina(n), struct(n), ktzio(n), ndrio(n), tedd(n), selt(n), sift(n), muse(n), pathto(n), scan(n), play(n), walk(n), reduce(n), formats(n), stan(n)

### AUTHORS

> Bernard Berthomieu, LAAS/CNRS, 2000-2026, Bernard.Berthomieu@laas.fr.

Tina Tools | plan (n) | Version 4.0.0

Generated by manServer 1.07 from src/plan.n using man macros.